{"text_format":"3","workbook":"xlsx","n_sheets":14,"sheets":["汇总","搪玻璃设备","不锈钢非标设备","离心机","螺带干燥机","气流粉碎机","冷水机组 ","闪蒸烘干机","物料输送系统","玻璃钢、PP设备","石墨冷凝器","泵类","过滤器","其它单项设备"],"not_rendered":{"images":3},"read":"whole","date_system":"1900"}

{"sheet":"汇总","index":0,"n_rows":32,"n_cols":4,"rows_kept":32,"merged":[[0,0,0,3],[1,0,1,3],[2,0,2,3]]}
["海森药业新区部分设备汇总表"]
["注：汇总数量为设计规划暂定数量，采购时部分将按需调整。"]
["需求状态说明：设备数量、清单已大致框定（规格型号、详细图集待定）。"]
["名称","单位","总量","备注"]
["搪玻璃设备","台",210]
["不锈钢非标设备","台",599]
["离心机","台",29]
["混合、干燥设备","台",24]
["气流粉碎机","台",4]
["冷水机组","台",12]
["闪蒸烘干机","台",2]
["物料输送系统（各分项设备约56台）","套",3]
["玻璃钢、PP设备","台",15]
["石墨冷凝器","台",22]
["泵类","台",344]
["过滤器","台",35]
["锥形整粒机","台",8]
["纳滤膜组","台",1]
["膜脱水处理系统","台",1]
["吡啶初蒸设备","台",2]
["三级尾气吸收系统","台",1]
["冷却塔","台","待定"]
["空调机组洁净房","台",3]
["空压机","台",4]
["制氮机组","台",1]
["纯化水设备","台",2]
["空调机组","台",3]
["智能分层仪","台",14]
["分层缓冲罐","台",2]
["自动取样pH检测","台",4]
["防腐手套箱","台",1]
["合计：",null,{"$f":"SUM(C5:C31)","v":1346}]

{"sheet":"搪玻璃设备","index":1,"n_rows":34,"n_cols":7,"rows_kept":34,"merged":[[0,0,0,2],[2,0,12,0],[2,1,12,1],[13,0,28,0],[13,1,28,1],[29,0,30,0]]}
["新区",null,null,"一车间","二车间","三车间","四车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套","数量/台套","数量/台套"]
["反应釜","搪玻璃","12500L",2,null,2,8]
[null,null,"10000L",8,null,10]
[null,null,"8000L",6,7,null,9]
[null,null,"6300L",8,null,11,15]
[null,null,"5000L",10,10,3,5]
[null,null,"4000L",{"$nulls":3},1]
[null,null,"3000L",5,7]
[null,null,"2000L",3]
[null,null,"1500L",null,1]
[null,null,"1000L",null,1]
[null,null,"500L",1]
["槽类","搪玻璃","20000L",null,null,1]
[null,null,"15000L",null,null,6]
[null,null,"12500L",null,null,1]
[null,null,"10000L",null,1,null,1]
[null,null,"8000L",null,1]
[null,null,"6300L",null,4,null,3]
[null,null,"5000L",1,6,4,2]
[null,null,"4000L",2,null,null,1]
[null,null,"3000L",4,1]
[null,null,"2500L",{"$nulls":3},1]
[null,null,"2000L",null,3,2]
[null,null,"1500L",null,2]
[null,null,"1000L",7,5,1]
[null,null,"800L",1]
[null,null,"500L",1,2]
[null,null,"200L",null,2,null,2]
["精馏塔","搪玻璃",{"$nulls":3},1]
[null,"搪玻璃","6300L",null,null,3]
["冷凝器","搪玻璃","30m2",null,null,3]
["过滤器","搪玻璃","100L",null,null,2]
[null,null,"合计",{"$f":"SUM(D3:D33)","v":59},{"$f":"SUM(E3:E33)","v":53},{"$f":"SUM(F3:F33)","v":50},{"$f":"SUM(G3:G29)","v":48}]

{"sheet":"不锈钢非标设备","index":2,"n_rows":85,"n_cols":9,"rows_kept":85,"merged":[[0,0,0,2],[0,7,0,8],[2,0,53,0],[2,1,7,1],[8,1,34,1],[35,1,37,1],[41,1,42,1],[43,1,49,1],[51,1,52,1],[54,0,60,0],[54,1,60,1],[61,0,66,0],[61,1,66,1],[67,0,72,0],[67,1,70,1],[71,1,72,1],[76,1,78,1]]}
["新区",null,null,"一车间","二车间","三车间","四车间"," 罐区设备"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套","数量/台套","数量/台套","数量/台套","尺寸"]
["槽类","不锈钢带夹套","5000L",null,null,2]
[null,null,"4000L",2]
[null,null,"3000L",1]
[null,null,"1000L",1]
[null,null,"800L",null,null,3]
[null,null,"500L",3]
[null,"不锈钢","100000L",{"$nulls":3},1,2,"4800*6000"]
[null,null,"50000L",{"$nulls":4},25,"3600*6000"]
[null,null,"45000L",{"$nulls":3},1]
[null,null,"40000L",{"$nulls":4},3,"3600*4000"]
[null,null,"30000L",4,{"$nulls":3},9,"2800*6000"]
[null,null,"25000L",null,1]
[null,null,"20000L",5,1]
[null,null,"18000L",{"$nulls":3},3]
[null,null,"15000L",null,null,1,3]
[null,null,"12000L",{"$nulls":3},2]
[null,null,"10000L",15,5,8,9]
[null,null,"8000L",4,14,1]
[null,null,"6000L",null,4,5]
[null,null,"5000L",16,8,8,3]
[null,null,"4000L",1,null,1]
[null,null,"3500L",{"$nulls":3},5]
[null,null,"3000L",12,14,7]
[null,null,"2500L",2]
[null,null,"2000L",12,14,4,4]
[null,null,"1500L",13,4,5,12]
[null,null,"1000L",7,3,19,5]
[null,null,"800L",null,null,1,2]
[null,null,"500L",8,7,4,4]
[null,null,"300L",8,1,5]
[null,null,"200L",4]
[null,null,100,1]
[null,null,50,1,1]
[null,"碳钢","95000L",{"$nulls":4},2,"3600*8000"]
[null,null,"200000L",null,null,2]
[null,null,"50000L",{"$nulls":4},1,"3600*6000"]
[null,null,"10000L",null,null,1]
[null,null,"8000L",null,1]
[null,null,"1200L",null,null,1]
[null,"钛","2200L",{"$nulls":3},5]
[null,null,500,{"$nulls":3},1]
[null,"钢衬po","50000L",{"$nulls":3},1]
[null,null,"20000L",null,1]
[null,null,"10000L",null,2]
[null,null,"6000L",null,1]
[null,null,"5000L",null,2]
[null,null,"8000L",{"$nulls":3},2]
[null,null,"2500L",{"$nulls":3},6]
[null,"钢衬PU","800000L",{"$nulls":4},2,"4200*6000"]
[null,"钢衬胶","50000L",{"$nulls":3},3]
[null,null,"10000L",{"$nulls":3},3]
[null,"制氨槽(带盘管)","15000L",{"$nulls":3},2]
["反应釜","不锈钢","6300L",null,null,6]
[null,null,"6000L",null,null,3]
[null,null,"5000L",1,4,6,2]
[null,null,"3000L",null,3,4]
[null,null,"2000L",null,5,1]
[null,null,"1500L",null,3,1]
[null,null,"200L",null,null,1]
["冷凝器","不锈钢","40㎡",null,null,9]
[null,null,"30㎡",3,null,7]
[null,null,"20㎡",11,null,5]
[null,null,"10㎡",10,null,7]
[null,null,"6㎡",1]
[null,null,"5㎡",3]
["螺旋板式冷凝器","不锈钢","30㎡",4,8]
[null,null,"20㎡",3,17]
[null,null,"10㎡",14]
[null,null,"5㎡",10]
[null,"碳化硅","30㎡",null,6]
[null,null,"20㎡",null,9]
["列管式冷凝器","不锈钢","40㎡",4]
["精馏塔系统","不锈钢",null,9,1]
["精馏塔","不锈钢","500×5000",4]
["萃取塔","待设计",{"$nulls":3},2]
["水相连续萃取塔",{"$nulls":4},2]
["油相连续水洗塔",{"$nulls":4},2]
["吡啶脱水塔","不锈钢",{"$nulls":4},1]
["甲醇回收塔","钛",{"$nulls":4},1]
["吸收塔","钛","直径500",{"$nulls":3},1]
["精馏降膜蒸发器","316L","50m2",null,null,1]
["薄膜蒸发器",304,"20m3",null,null,1]
[null,null,"合计",{"$f":"SUM(D3:D82)","v":197},{"$f":"SUM(E3:E84)","v":140},{"$f":"SUM(F3:F84)","v":136},{"$f":"SUM(G3:G82)","v":82},{"$f":"SUM(H3:H82)","v":44}]

{"sheet":"离心机","index":3,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[0,0,0,2],[2,0,6,0],[3,1,4,1],[5,1,6,1]]}
["新区",null,null,"一车间","二车间","三车间","四车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套","数量/台套","数量/台套"]
["下卸料离心机","内衬",1600,null,5]
[null,304,1600,5,5]
[null,null,1250,null,null,7]
[null,"316L",1000,{"$nulls":3},1]
[null,null,1600,4,null,null,7]
[null,null,"合计",{"$f":"SUM(D5:D7)","v":4},10,7,{"$f":"SUM(G5:G7)","v":8}]

{"sheet":"螺带干燥机","index":4,"n_rows":14,"n_cols":7,"rows_kept":14,"merged":[[0,0,0,2],[2,0,4,0],[6,0,10,0],[8,1,10,1]]}
["新区",null,null,"一车间","二车间","三车间","四车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套","数量/台套","数量/台套"]
["螺带混合机",2507,"1500L",null,1]
[null,"316L","4000L",1]
[null,304,"5000L",null,null,1]
["单锥混合机","316L","3000L",{"$nulls":3},1]
["螺带干燥机",2507,"1500L",null,2]
[null,"316L","1500L",5]
[null,304,"2000L",null,1]
[null,null,"1500L",2,4]
[null,null,"4000L",2]
["螺带回转真空干燥机",304,"5000L",null,null,1]
["单锥干燥机","搪玻璃","1000L",null,1]
[null,null,"合计",{"$f":"SUM(D4:D12)","v":10},{"$f":"SUM(E3:E13)","v":9},2,3]

{"sheet":"气流粉碎机","index":5,"n_rows":6,"n_cols":6,"rows_kept":6,"merged":[[0,0,0,2]]}
["新区",null,null,"一车间","三车间","四车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套   ","数量/台套"]
["气流粉碎机","316L","150KG/小时",null,null,2]
["气流粉碎机","316L","＞80kg/h",1]
["气流粉碎机",304,"200~300kg/h",null,1]
[null,null,"合计",{"$f":"SUM(D3:D4)","v":1},1,{"$f":"SUM(F3:F4)","v":2}]

{"sheet":"冷水机组 ","index":6,"n_rows":9,"n_cols":3,"rows_kept":9,"merged":[[0,0,0,1],[3,0,4,0],[5,0,6,0]]}
["新区",null,"动力车间"]
["设备名称","制冷量","数量/台套   "]
["负20度蒸发冷螺杆冷水机组","1034KW（制冷）",2]
["7度蒸发冷螺杆冷水机组","1352KW（制冷）",2]
[null,"993KW（制冷）",2]
["5度蒸发冷螺杆冷水机组","922KW（制冷）",2]
[null,"414KW（制冷）",2]
["负30度蒸发冷螺杆冷水机组","300KW（制冷）",2]
[null,"合计",{"$f":"SUM(C3:C8)","v":12}]

{"sheet":"闪蒸烘干机","index":7,"n_rows":5,"n_cols":4,"rows_kept":5,"merged":[[0,0,0,2],[2,0,3,0],[2,1,3,1]]}
["新区",null,null,"四车间"]
["设备名称","材质","规格型号","数量/台套"]
["闪蒸烘干机","316L","600KG/小时",1]
[null,null,"100kg/h",1]
[null,null,"合计",2]

{"sheet":"物料输送系统","index":8,"n_rows":15,"n_cols":6,"rows_kept":15,"merged":[[0,0,0,2]]}
["新区",null,null,"一车间","三车间","四车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套","数量/台套"]
["铝片投料器","不锈钢",{"$nulls":3},12]
["密闭投料箱（活性炭）",{"$nulls":4},4]
["自动出料活性炭过滤器（烛式）","316或双相钢",{"$nulls":3},3]
["自动取样器","316L",{"$nulls":3},7]
["固体物料输送、混合、包装系统",{"$nulls":4},2]
["洁净区自动称量包装系统","316L",null,1]
["洁净区固体物料自动化管道输送系统","316L",null,1]
["密闭输送系统",304,null,3]
["湿品料真空输送系统",{"$nulls":4},2]
["真空上料机",304,null,11]
["密闭投料器",304,null,5,2,2]
["物料提升机",{"$nulls":4},1]
[null,null,"合计",{"$f":"SUM(D3:D13)","v":21},2,{"$f":"SUM(F3:F14)","v":33}]

{"sheet":"玻璃钢、PP设备","index":9,"n_rows":8,"n_cols":6,"rows_kept":8,"merged":[[0,0,0,2]]}
["新区",null,null,"一车间","四车间"," 罐区设备"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套","数量/台套"]
["脱氨塔",{"$nulls":3},1]
["喷淋塔",null,null,2]
["吸收塔",{"$nulls":4},6]
["降膜吸收器","PP","20㎡，四级吸收",2,3]
["吸附装置",null,null,1]
[null,null,"合计",{"$f":"SUM(D3:D7)","v":5},{"$f":"SUM(E3:E7)","v":4},{"$f":"SUM(F5:F7)","v":6}]

{"sheet":"石墨冷凝器","index":10,"n_rows":7,"n_cols":5,"rows_kept":7,"merged":[[0,0,0,2],[2,0,5,0],[2,1,5,1]]}
["新区",null,null,"三车间","四车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套"]
["石墨冷凝器","石墨","40㎡",4]
[null,null,"30㎡",1]
[null,null,"20㎡",1,12]
[null,null,"10㎡",4]
[null,null,"合计",{"$f":"SUM(D3:D6)","v":10},{"$f":"SUM(E3:E5)","v":12}]

{"sheet":"泵类","index":11,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[0,0,0,2]]}
["新区",null,null,"一车间","二车间","四车间"," 罐区设备"]
["设备名称","材质","规格型号","数量/台套   ","数量","数量/台套","数量/台套"]
["各类泵",null,null,34,130,33,82]
["蠕动泵","不锈钢",null,11,null,24]
[null,"衬四氟",{"$nulls":3},4]
["真空泵","不锈钢",null,24]
["螺杆泵","不锈钢",null,2]
[null,null,"合计",{"$f":"SUM(D3:D7)","v":71},130,{"$f":"SUM(F3:F7)","v":61},82]

{"sheet":"过滤器","index":12,"n_rows":11,"n_cols":7,"rows_kept":11,"merged":[[0,0,0,2],[3,0,6,0],[5,1,6,1]]}
["新区",null,null,"一车间","二车间","三车间","四车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套   ","数量/台套","数量/台套"]
["过滤器","不锈钢",null,1]
["精密过滤器","不锈钢",null,5,null,null,3]
[null,304,"50L",null,9,1]
[null,"钛","5芯",{"$nulls":3},4]
[null,null,"7芯",{"$nulls":3},4]
["袋式过滤器","不锈钢",null,3,2,null,1]
["烛式过滤器",{"$nulls":5},1]
["压滤过滤器",304,"500L",null,null,1]
[null,null,"合计",{"$f":"SUM(D3:D8)","v":9},{"$f":"SUM(E3:E8)","v":11},2,{"$f":"SUM(G3:G9)","v":13}]

{"sheet":"其它单项设备","index":13,"n_rows":20,"n_cols":6,"rows_kept":20,"merged":[[0,0,0,2],[2,0,3,0],[10,0,11,0],[13,0,14,0]]}
["新区",null,null,"一车间","四车间","动力车间"]
["设备名称","材质","规格型号","数量/台套   ","数量/台套","数量/台套"]
["锥形整粒机",304,null,2]
[null,"316L",null,1,5]
["纳滤膜组",{"$nulls":3},1]
["膜脱水处理系统",null,null,1]
["吡啶初蒸设备","钛2","500Kg/h,4吨/天",null,2]
["三级尾气吸收系统",{"$nulls":3},1]
["冷却塔",{"$nulls":4},"待定"]
["空调机组洁净房",{"$nulls":3},3,"待定"]
["空压机",null,"20M3/min,压力0.5PMA  75KW",null,null,2]
[null,null,"20M3/min ,压力0.8PMA 110KW ",null,null,2]
["制氮机组 ",null,"制氮量400NM3/H，纯度≥99.5",null,null,1]
["纯化水设备","30M3/H","原水泵15KW+一级高压泵37KW+二级高压泵30KW+送出纯水泵11KW ，合计93KW",null,null,1]
[null,"10M3/H","原水泵7.5KW+一级高压泵15KW+二级高压泵15KW+送出纯水泵11KW ，合计37.5KW",null,null,1]
["智能分层仪","不锈钢",null,14]
["分层缓冲罐","5L",null,null,2]
["自动取样pH检测","不锈钢",null,4]
["防腐手套箱",null,null,1]
[null,null,"合计",{"$f":"SUM(D5:D19)","v":20},{"$f":"SUM(E5:E19)","v":9}]